bit One HD Virtuoso Beta Release Notes 3.1: 

1) Automatic selection of S/Pdif Optical 2 input with audio carrier recognition. Available only on Virtuoso rev.4.
2) Minox bug Fix.




bit One HD Virtuoso Beta Release Notes 3.0: 


1) Introduction of RTA measurement.
	A) Possibility of performing auto equalization after RTA acquisition.
	B) Editable or downloadable target curves.
	C) Import of equalization curves for front from REW.
2) Introduction of IIR Graphic Equalizer Mode.
3) Introduction of Dinamic Bass Boost.
4) Introduction of Dynamic EQ.
5) Introduction of All Pass on Channel EQ extended over the whole band.
6) All PASS extension on interface inputs 0-180 first order and 0-360 second order.
7) New submenu "Outputs Configuration Wizards".
        A) Management change on "I / O Configuration Wizard" Pop Up.
	B) All Pass analysis always enabled.
	C) AC LINK Select ALL.
9) Add "Virtuoso" Power On from PC Software connection.
10) MPC Percept® algorithm, usable with bit Tune interfacing.
11) Automatic selection of S/Pdif Optical 1 input with audio carrier recognition.
12) Channel EQ graphic display update, with introduction of the trend of the edge phase.
13) Visualization of the Phase, in the front equalizer.
14) Graphic modification end of set RT.
15) (Audison Data Control) ex SDC (Serial Data Control) serial port activation:
	a) Management of inputs and absolute volume with B-CON interface.
	b) Interfacing with W-CON device, for programming, bit One HD VIrtuoso interfacing.
This feature is only available for the bit One HD Virtuoso processors.
16) Minox bug Fix.


 
Note:
This software is compatible with FW. 3.0.0.xx or higher
 
  

  V 2.0.3  GUI Upgrades:
       -I/O configuration Wizard, using the USB Setup dongle
	

     
 V 2.0.2

        1. Sound tuning: Automatic De-equalization improved by introducing IIR equalization pole in the 20-100 Hz area
        2. Graphic enhancements.
	3. Minor bug fixing.


NOTE:
New PC SW version v.2.0.2 is compatible with new FW version v.2.0.2.284.
The synchronization with device having old FW versions will be possible anyway but new functionality won't be available until the FW update is completed.



 V 2.0.1
 
	1. 	Automatic management of Bit One HD and Bit One HD Virtuoso Hardware.

	2.	 OEM integration and I/O configuration wizard
A: Optimized phase analysis with the possibility of using the 2nd order All Pass, and then checking and optimizing the linearization curve of the Master input using the "Total Electric Response" graph.
B: Manual management of the All Pass entry, with the possibility of using the 1st and 2nd order All Pass. Possibility to trace the resulting curve using the "Total Electric Response" graph.

	3. 	New time delay management from Pop-Up menu.

	
NOTE:
New PC SW version v.2.0.1 is compatible with new FW version v.2.0.1.277.
The synchronization with device having old FW versions will be possible anyway but new functionality won't be available until the FW update is completed.




 V 2.0 New features GUI/Firmware

	1.	OEM integration and I/O configuration wizard 
A.Implemented one FW only for both FIR or IIR digital network. 
B.Added Pass-through input configuration (MASTER) 
C.Added automatic polarity check of input speaker wires (MASTER) 
D.Improved De-EQ by introducing the De-Phase analysis (MASTER) 
E.of PASS THROUGH input setup, this step will only determine the crossover cut-off points of each input channels. 
F.Added Input analysis dashboard screen (MASTER) 
G.Expanded the output speaker configuration capability (output channel map) 

	2.	Sound tuning capabilities 
Added EQ poles and other capabilities. Main improvements concern the 3 main EQ: 

- Input EQ: 
A.IIR / FIR versions: from 3 PEQ (FIR) + 2 Shelving (FIR) to 8+1 PEQ (FIR+IIR) + 1 Hi-Shelf (FIR). 
B.II. Added the free selection of input fronts (FRONT L, FRONT R, REAR R, REAR R, CENTER, SUB) in order to unlink the input EQ. 
C.Added the 4 All-pass filters (2nd order) for each input fronts (FRONT L, FRONT R, REAR R, REAR R, CEN-TER, SUB) .
D.. IV. Added quick sensitivity level adjustments (MASTER) 3 stages (ref, +3dB, +6dB).

- Main EQ: 
A.IIR / FIR versions: from 3 PEQ (FIR) + 2 Shelving (FIR) to 4 PEQ (FIR) + 1 PEQ (IIR, up to 100Hz) + 1 high-Shelf (FIR) 
B.II. Added the selection of slow/ fast roll settings of DAC .

- Channels EQ, previously named as Output EQ: 
A.IIR version: from 9 PEQ + 2 Shelving (IIR) to 11 PEQ + 2 Shelving (IIR) 
B.FIR version: from 3 PEQ (FIR) + 2 Shelving (FIR) + 3 PEQ (IIR , up 500Hz) to 8 PEQ (FIR) + 1 Hi-Shelf (FIR) + 1 Lo-Shelf (IIR) + 2 PEQ (IIR , whole bandwidth) 
C.IIR/FIR version: added the Notch filters (IIR up to 3, FIR up to 2).
D.IIR / FIR versions: added the All-pass filters (1st or 2nd orders) , one for each x-over transition area cen-tred at the cut off freq. chosen.   
 

	3.	Graphic & User Interface 
A.Removed STANDARD working mode 
B.LIMITER function disabled by default 
C.Added battery status monitor 
D.Added filter settings (TA and X-over) pop-up window 
E.Added EQ settings pop-up window 
F.Improved keyboard layout compatibility and introduced new combos for EQ section 
G.Changed the EQ’s amplitude (dB ) default visualization and adjustment ranges 
H.Improved the EQ’s Q-factor adjustment range for peaking/notch filters. 
I.Added EQ control windows setting (parameters Fc, gain, Q) also when use FIR poles. 
J.Introduced config. menu for enabling/disabling AD/AC link outputs 
K.Graphic enhancements. 



Bug fixes :
 
1.GUI:TA alignment anomaly when set through a certain keyboard combination. 
2.FW:Fixed sporadic input source change (instability) when the bit One HD was powered on. 
3.FW:Reduced audio latency when use FIR EQ poles at low frequency. 
4.FW:Improved FIR EQ’s filters by reducing the ringing effects. 
5.FW:Fixed soft “click” noise when switch digital input sources with different sampling frequency. 
6.GUI:Corrected crossover graph visualization error plotted on EQ when Midrange was selected. 
7.GUI:Fixed EQ’s zoom anomaly that could shift EQ poles already set when switching from one equalizer to an-other. 
8.GUI:Expanded the release time range to 6.8 sec, available through the “Auto chime” function. 



it One HD Release Notes: 

V 2.0.3  GUI Upgrades:
       -I/O configuration Wizard, using the USB Setup dongle
	

     
 V 2.0.2

        1. Sound tuning: Automatic De-equalization improved by introducing IIR equalization pole in the 20-100 Hz area
        2. Graphic enhancements.
	3. Minor bug fixing.


NOTE:
New PC SW version v.2.0.2 is compatible with new FW version v.2.0.2.284.
The synchronization with device having old FW versions will be possible anyway but new functionality won't be available until the FW update is completed.



 V 2.0.1
 
	1. 	Automatic management of Bit One HD and Bit One HD Virtuoso Hardware.

	2.	 OEM integration and I/O configuration wizard
A: Optimized phase analysis with the possibility of using the 2nd order All Pass, and then checking and optimizing the linearization curve of the Master input using the "Total Electric Response" graph.
B: Manual management of the All Pass entry, with the possibility of using the 1st and 2nd order All Pass. Possibility to trace the resulting curve using the "Total Electric Response" graph.

	3. 	New time delay management from Pop-Up menu.

	
NOTE:
New PC SW version v.2.0.1 is compatible with new FW version v.2.0.1.277.
The synchronization with device having old FW versions will be possible anyway but new functionality won't be available until the FW update is completed.




 V 2.0 New features GUI/Firmware

	1.	OEM integration and I/O configuration wizard 
A.Implemented one FW only for both FIR or IIR digital network. 
B.Added Pass-through input configuration (MASTER) 
C.Added automatic polarity check of input speaker wires (MASTER) 
D.Improved De-EQ by introducing the De-Phase analysis (MASTER) 
E.of PASS THROUGH input setup, this step will only determine the crossover cut-off points of each input channels. 
F.Added Input analysis dashboard screen (MASTER) 
G.Expanded the output speaker configuration capability (output channel map) 

	2.	Sound tuning capabilities 
Added EQ poles and other capabilities. Main improvements concern the 3 main EQ: 

- Input EQ: 
A.IIR / FIR versions: from 3 PEQ (FIR) + 2 Shelving (FIR) to 8+1 PEQ (FIR+IIR) + 1 Hi-Shelf (FIR). 
B.II. Added the free selection of input fronts (FRONT L, FRONT R, REAR R, REAR R, CENTER, SUB) in order to unlink the input EQ. 
C.Added the 4 All-pass filters (2nd order) for each input fronts (FRONT L, FRONT R, REAR R, REAR R, CEN-TER, SUB) .
D.. IV. Added quick sensitivity level adjustments (MASTER) 3 stages (ref, +3dB, +6dB).

- Main EQ: 
A.IIR / FIR versions: from 3 PEQ (FIR) + 2 Shelving (FIR) to 4 PEQ (FIR) + 1 PEQ (IIR, up to 100Hz) + 1 high-Shelf (FIR) 
B.II. Added the selection of slow/ fast roll settings of DAC .

- Channels EQ, previously named as Output EQ: 
A.IIR version: from 9 PEQ + 2 Shelving (IIR) to 11 PEQ + 2 Shelving (IIR) 
B.FIR version: from 3 PEQ (FIR) + 2 Shelving (FIR) + 3 PEQ (IIR , up 500Hz) to 8 PEQ (FIR) + 1 Hi-Shelf (FIR) + 1 Lo-Shelf (IIR) + 2 PEQ (IIR , whole bandwidth) 
C.IIR/FIR version: added the Notch filters (IIR up to 3, FIR up to 2).
D.IIR / FIR versions: added the All-pass filters (1st or 2nd orders) , one for each x-over transition area cen-tred at the cut off freq. chosen.   
 

	3.	Graphic & User Interface 
A.Removed STANDARD working mode 
B.LIMITER function disabled by default 
C.Added battery status monitor 
D.Added filter settings (TA and X-over) pop-up window 
E.Added EQ settings pop-up window 
F.Improved keyboard layout compatibility and introduced new combos for EQ section 
G.Changed the EQ’s amplitude (dB ) default visualization and adjustment ranges 
H.Improved the EQ’s Q-factor adjustment range for peaking/notch filters. 
I.Added EQ control windows setting (parameters Fc, gain, Q) also when use FIR poles. 
J.Introduced config. menu for enabling/disabling AD/AC link outputs 
K.Graphic enhancements. 



Bug fixes :
 
1.GUI:TA alignment anomaly when set through a certain keyboard combination. 
2.FW:Fixed sporadic input source change (instability) when the bit One HD was powered on. 
3.FW:Reduced audio latency when use FIR EQ poles at low frequency. 
4.FW:Improved FIR EQ’s filters by reducing the ringing effects. 
5.FW:Fixed soft “click” noise when switch digital input sources with different sampling frequency. 
6.GUI:Corrected crossover graph visualization error plotted on EQ when Midrange was selected. 
7.GUI:Fixed EQ’s zoom anomaly that could shift EQ poles already set when switching from one equalizer to an-other. 
8.GUI:Expanded the release time range to 6.8 sec, available through the “Auto chime” function. 


----------------------------------------------------------------------------------------------------------

bit One HD Virtuoso Beta Release Notes 3.1: 


1) Selezione automatica ingresso  S/Pdif Optical 2 con riconoscimento portante audio. Disponibile solo su Virtuoso rev.4.
2) Correzzione bug minori.



bit One HD Virtuoso Beta Release Notes 3.0: 
1) Introduzione misura RTA.
	A) Possibilità di effetture dopo aqcuisizione RTA auto equalizzazione. 
	B) Curve Target editabili o scaricabili.
	C) Importazione curve di equalizzazione per fronte  da REW.
2) Introduzione Modalità equalizzatore grafico IIR
3) Introduzione Dinamic Bass Boost.
4) Introduzione Dynamic EQ.
5) Introduzione All Pass on Channel EQ esteso su tutta la banda.
6) Estensione All PASS su interfaccia ingressi 0-180 primo ordine e 0-360 secondo ordine.
7) Nuovo sotto menù “Outputs Configuration Wizards”.
        A) Modifica gestione su Pop Up “I/O Configuration Wizard”.
	B) All Pass analysis sempre abilitata.
	C) AC LINK Select ALL.
9) Inserimento "Virtuoso" Power On da collegamento PC Software.
10) Algoritmo MPC Percept®, fruibile con interfacciamento  bit Tune.
11) Selezione automatica ingresso  S/Pdif Optical 1 con riconoscimento portante audio.
12) Aggiornamento visualizzazione grafica Channel EQ, con introduzione visualizzazione dell'andamento della Fase dei fronti.
13) Visualizzazione andamento della Fase nell equalizzatore di fronte.
14) Modifica grafica fine set RT.
15) Attivazione porta seriale ADC (Audison Data Control) ex SDC (Serial Data Control):
	a)Gestione Ingressi e absolute Volume con interfacciamento Audison B-CON .
	b)Interfacciamento con dispositivo Audison W-CON, per programmazione, interfacciamento del bit One HD VIrtuoso.
Questa funzione è disponibile solo per i processori bit One HD Virtuoso.
16) Correzzione bug minori.


Nota:
Questo Software è compatibile con FW. 3.0.0.xx o superiore

 
 
 
V 2.0.3 Aggiornamenti GUI:
        -I/O configurazione Guidata, con l'utilizzo della dongle USB Setup.



 V 2.0.2 Aggiornamenti GUI/Firmware.

        1.  Sound Tuning: Migliorata la De-Equalizzazione automatica introducendo polo equalizzazione IIR nella zona 20-100 Hz.
        2.  Miglioramenti grafici.
        3.  Minor bug fixing.


NOTA:
La nuova versione SW per PC v.2.0.2 è compatibile con la nuova versione FW v.2.0.2.284.
La sincronizzazione con un dispositivo con versioni FW precedenti sarà comunque possibile, ma le nuove funzionalità non saranno disponibili fino al completamento dell'aggiornamento FW.


  V 2.0.1 Aggiornamenti GUI/Firmware.


	1.       Gestione automatica del Software di Hardware  bit One HD e bit One HD Virtuoso.

	2.	 I/O configurazione guidata ed integrazione OEM
A: Ottimizzata analisi di fase con la possibilità di utilizzare All Pass  di 2° ordine, e verificare e ottimizzare successivamente la curva di linearizzazione dell'ingresso Master tramite il grafico "Total Electric Response".
B: Gestione manuale degli All Pass di ingresso , con la possibilità di utilizzare All Pass di 1° e 2° ordine. Possibilità di tracciare la curva risultante tramite il grafico "Total Electric Response".

	3.       Nuova gestione ritardi temporali da menù Pop-Up.
 

NOTA:
La nuova versione SW per PC v.2.0.1 è compatibile con la nuova versione FW v.2.0.1.277.
La sincronizzazione con un dispositivo con versioni FW precedenti sarà comunque possibile, ma le nuove funzionalità non saranno disponibili fino al completamento dell'aggiornamento FW.


V 2.0 Aggiornamenti GUI/Firmware.

      1.	I/O configurazione guidata ed integrazione OEM
A.Unificato il FW per supportare entrambe le reti digitali FIR ed IIR.
B.Aggiunta configurazione d’ingresso Pass-Through (MASTER)
C.Aggiunto verifica automatica della polarità di ingresso dell'altoparlante (MASTER)
D.Migliorata la De-Equalizzazione introducendo l’analisi in fase (MASTER)
E.Aggiunta pannello di analisi degli ingressi, dashboard (MASTER).
F.Ampliata la configurazione massima d’uscita (mappa dei canali di uscita).

      2.	 Sound Tuning 
Aggiunti poli EQ e altre funzionalità. I miglioramenti riguardano i 3 equalizzatori principali elencati :

- Input EQ : 
A.Versioni IIR / FIR: da 3 PEQ (FIR) + 2 Shelving (FIR) a 8 + 1 PEQ (FIR + IIR) + 1 Hi-Shelf (FIR). 
B.aggiunta la selezione libera dei fronti di ingresso (FRONT L, FRONT R, REAR R, REAR R, CENTER, SUB) per scollegare l'EQ di input. 
C.aggiunti 4 filtri passa tutto (All-pass) del 2° ordine per ciascun fronte d’ingresso (FRONT L, FRONT R, REAR R, REAR R, CENTER, SUB) .
D.aggiunte regolazioni veloci del livello di sensibilità (MASTER) 3 livelli (ref, + 3dB, +6 dB).

- Main EQ: 
A.Versioni IIR / FIR : da 3 PEQ (FIR) + 2 Shelving (FIR) a 4 PEQ (FIR) + 1 PEQ (IIR, fino a 100Hz) + 1 high-Shelf (FIR) 
B.Aggiunta la selezione delle impostazioni del filtro di uscita dei convertitori DAC,  scelta tra “Fast roll-off” e “Slow roll-off”.

- Channels EQ, precedentemente denominato Output EQ: 
A.Versione IIR : da 9 PEQ + 2 Shelving (IIR) a 11 PEQ + 2 Shelving (IIR) 
B.Versione FIR : da 3 PEQ (FIR) + 2 Shelving (FIR) + 3 PEQ (IIR, fino a 500Hz) a 8 PEQ (FIR) + 1 Hi- Shelf (FIR) + 1 Lo-Shelf (IIR) + 2 PEQ (IIR, su tutta la larghezza di banda) 
C.IIR / FIR versione : aggiunti i filtri Notch (IIR fino a 3, FIR fino a 2)
D.Versioni IIR / FIR : aggiunti filtri passa tutto (all-pass) del 1° o 2° ordine, uno per ogni area di transizione del filtro x-over centrato esattamente alla frequenza taglio scelto. 

      3.	Interfaccia utente e grafica 
A.Eliminata la modalità di lavoro STANDARD
B.Funzione LIMITER disabilitata di default 
C.Aggiunto voltmetro per il monitoraggio della tensione batteria 
D.Aggiunta finestra pop-up per le impostazioni del filtro (TA e X-over) 
E.Aggiunta finestra pop-up per le impostazioni EQ .
F.Migliorata compatibilità nell’uso della tastiera ed introdotte nuove combinazioni per la sezione EQ 
G.Modificato l'intervallo di visualizzazione e di regolazione dell'ampiezza (dB) dell'equalizzatore EQ 
H.Miglioramento del campo di regolazione del fattore Q dell'EQ per i filtri parametrici. 
I.Aggiunta finestra di controllo dei parametri dei poli di EQ (parametri Fc, guadagno, Q) anche quando si usano poli tipo FIR. 
J.Introdotto menu di config. per l’abilitazione/disabilitazione delle uscite AD/AC link 
K.Miglioramenti grafici.



Bug risolti:

1.GUI: Anomalia nell’esecuzione dei ritardi temporali (TA) quando venivano impostati da tastiera con una determi-nata combinazione di tasti. 
2.FW:Sporadico cambio sorgente (rispetto alla selezione prima dello spegnimento) quando il bit One HD veniva riacceso. 
3.FW:Ridotta la latenza audio quando si usano i poli FIR EQ a bassa frequenza. 
4.FW:Miglioramento dei filtri di Equalizzazione FIR, riducendo gli effetti di “Ringing”. 
5.FW:Risolto il problema del rumore tipo "click", quando si commuta tra sorgenti di ingresso digitali che riproduco-no brani con frequenza di campionamento diversa. 
6.GUI:Corretto piccolo errore di visualizzazione grafica della curva crossover, visualizzata nella schermo EQ, quando il Midrange veniva selezionato. 
7.GUI:Anomalia della funzione zoom del grafico equalizzatore, che se usata poteva traslare leggermente i poli già impostati quando si passava da un equalizzatore ad un altro. 
8.GUI:Esteso l'intervallo per il tempo di rilascio (release time) fino a 6,8 secondi, per la funzione “Auto chime”. 




